List of NorBuild changes:

Version 4.2.33, 21.10.2020

Version 4.2.32, 17.04.2019
• Knauf Spezial: Menu item «Luftschallkorr. V3.0.74 Knauf» in order to correct impact with airborne acc. to DIN 4109 instead of ISO 10140
• Trittschall mit Luftschall: Im Fall Luftschallabstand < 3dB Korrektur um 3 dB realisieren statt bisher keine Korrektur
• Trittschall mit Luftschall: Umbenennung von LHW in LTS und LE in Li für ISO 10140
• FIxed: Some Excel template files contained broken data.

Version 4.2.31, 07.03.2019
• Fixed: ISO 16283-3 Facade Loudspeaker Airborne low freq. (corner) didn't take into account the low freq procedure.

Version 4.2.30, 21.01.2019
• Compressed and squized printout fixed (mainly under Windows 10.
• Shifted ref. curve error fixed for Laboratory ASTM Impact in Excel export.

Version 4.2.29, 26.11.2018
• Indicate background noise limits in test report with ?, ?, < signs. Applies to NorBuild and Excel.

Version 4.2.28, 28.05.2018
• libxl 3.8.2.0
• Code Sign Certificate from COMODO
• HASP dongle driver updated
• New installer (NorBuildSetup.exe)

Version 4.2.27, 13.11.2017
• Nor150 support of Intensity mode files

Version 4.2.26, 18.09.2017
• BS EN ISO 16283-2 (BB93 Reg E4)

Version 4.2.25, 22.03.2017
• SS 25267:2015 (DnT,w,50; DnT,w,100; LnTw50; LnTw20: only available in Excel export)

Version 4.2.24, 08.12.2016
• Nor150 support for all modes

Version 4.2.22, 07.11.2016
• Release version

Version 4.2.20, 06.09.2016
• ISO 16283-1: Amd1 max(S, V/7.5)
• DIN 4109-4
• Impact with airborne supports multiple positions
• Nor150 support

Version 4.1.19, 19.05.2016
• ÖNORM EN ISO 16283

Version 4.1.18, 08.02.2016
• ISO 16283-3 final release
• SIA 2006 updated for 16283-3
• ASTM E336-16 updated (suffix)

Version 4.1.17, 15.01.2016
• Missing Excel templates for ISO 16283-2 multi added
• Crash fixed when opening the Result table for low frequency (corner) projects

Version 4.1.16, 07.01.2016
• ISO 16283-2 final release
• BS EN ISO 16283-1 (BB93 Reg E4)
• ASTM E1007-14 and E336-14 updated (suffix)

Version 4.0.112, 17.08.2015
• Support for NorXfer v6
• Tested with Windows 10

Version 4.0.111, 31.03.2015
• C values calculation always based on 1 dB step index
• Impact airborne correction acc. to ISO 10140-3:2010 AM1:2014

Version 4.0.110, 04.12.2014
• Area of common partition for ISO 16283-1 DnT projects
• Error in channel description fixed in case of direct icon access and button Finish (NorMeasTool)
• Export multiple loudspeaker results to Excel (incl. templates)
• If Bgn exceeds signal - correction of -1.3 is applied as it used to be in the beginning of NorBuild
• Show T and Room Corr for Multiple Loudspeaker in result table
• LibXL version 3.6.1.0 update
• Result table refresh for BGN status when Multiple Loudspeaker fixed
• Loudspeaker averaging for SIA Airborne acc. to ISO 16283-1. Impact is prepared but put in comment.
• Error fixed for multiple export in case of .xlsm template
• Check number of sheets in the Excel template and adjust the required index if out of bounds

Version 4.0.109, 13.10.2014
• Multiplot crash fixed

Version 4.0.108, 17.09.2014
• Release version

Version 4.0.106, 10.09.2014
• Result table with detailed results for loudspeaker positions L#A..L#I
• Selection of loudspeaker positions L#A..L#I in the measurement table (ISO 16283, ISO 10140)
• ISO/DIS 16283-3, Facade incl. corner
• ISO/DIS 16283-2 for tapping machine positions, incl. Excel templates
• Support of Nor131, Nor132

Version 3.1.97, 16.06.2014
• ISO 16283-1 for Single loudspeaker positions, incl. Excel templates
• ISO 10140-2 Excel templates for Single loudspeaker positions added
• BS: Don't calc bgn corr for each mic position anymore - do it for each average (same mic position)


Version 3.1.96, 28.05.2014
• Support for *.xlsm Excel file templates


Version 3.1.95, 22.05.2014
• New ISO 16283-1, normal and low frequency (corner) procedure
• Geberit Spezial


Version 3.1.94, 11.11.2013
• New ISO 717:2013,  1/10 dB steps rating (except spectrum adaptation terms)
• New ISO/DIS 16283-1,  normal and low frequency (corner) procedure
• New ISO/DIS 16283-2,  normal and low frequency (corner) procedure
• ISO 15186-2,  Intensity standard
• ASTM standards 
• Windows 8 (x86, x64) support
• Excel templates based on .xlsx format
• Option system renamed: Absorption is now part of the “Advanced” option. This option includes Absoprtion and Intensity.
• Minor bug fixes and improvements


Version 3.0.73, 02.11.2011
• Windows 7(x86, x64) compability
• MS Office 2010 compability
• Minor bug fixes and improvements
• Support of the new laboratory Standard ISO 10140-x
• Support of the new national impact Standard NF S 31-074
• Support of Nor140 v2.1 when using the CtrlBuild optional feature for remote control
• Modified procedure to correct for bgn noise when the difference is 10.0 dB
• Possibility to specify a free text for reporting too high background noise







